**Computer Networking**

**Basics:**

* **Network**: A computer network is a digital telecommunications network for sharing resources between nodes, which are computing devices that use a common telecommunications technology
* **Node**: A computing device.
* **Bus network**: All the devices are connected on one single long cable.
* **Client**: A client is a piece of computer hardware or software that accesses a service available by a server
* **Server**: A server is a computer program or device that provides functionality for other programs or devices called clients
* **Protocol**: A set of rules used in communication between clients

**Network Devices:**

* **Repeater**: A repeater is an electronic device that receives a signal and retransmits it.
* **Hub**: A hub is essentially a multi-port repeater. Wireless Access Point is essentially a hub in the air
  + Active Hub: These are the hubs that have their own power supply and can clean, boost, and relay the signal along with the network. It serves both as a repeater as well as a wiring center.
  + Passive Hub: These are the hubs that collect wiring from nodes and power supply from the active hub. They are generally used to relay signals with cleaning or boosting them
  + Intelligent Hub: It works like active hubs and includes remote management capabilities. They also provide flexible data rates to network devices. It also enables an administrator to monitor the traffic passing through the hub and to configure each port in the hub.
* **Bridge**: A bridge is a repeater with add on the functionality of filtering content by reading mac addresses of source and destination. It was mostly used to interconnect two LANs.
  + Transparent Bridge: These are the bridges in which the stations are completely unaware of the bridge's existence.
  + Source Routing Bridge: In these bridges, routing operation is performed by the source station and the frame specifies the route to follow.
* **Switch**: A switch reads each frame and has the intelligence to transmit data to the port it is destined for.
* **Router**: A router is a device like a switch that routes data packets based on their IP addresses. The router is mainly a Network Layer device.
* **Wireless Access Point**: A wireless access point is a networking device that allows wireless-capable devices to connect to a wired network.
* **Wireless LAN Controller**: A WLAN controller is used to manage large scale deployments of light weight and normal wireless access points.
* **Firewall**: A firewall is a network security system that monitors and controls incoming and outgoing network traffic based on predetermined security rules.
* **IDS**: It’s a software system that warns if there is an intrusion. They just get copies of packets that are analyzed.
* **IPS**: It’s a software system can alert you if there may be a problem and block the same. They stay inline of the network and detect and block intrusions.
* **Email Security Appliance**: The Email Security Appliance is an email security gateway product. It is designed to detect and block a wide variety of email-borne threats, such as malware, spam and phishing attempts.
* **Load Balancer**: A load balancer is a device that acts as a reverse proxy and distributes network or application traffic across several servers.

**Types of Networks based on Area:**

* WAN: A Wide Area Network is a telecommunications network that extends over a large geographical area for the primary purpose of computer networking.
* LAN: A Local Area Network is a computer network that interconnects computers within a limited area such as a residence, school and so on
* MAN: Metropolitan Area Network
* Wireless Local Area Network (WLAN)
* Campus Area Network (CAN)
* Storage Area Network (SAN)
* Passive Optical Local Area Network (POLAN)
* Enterprise Private Network (EPN)
* Virtual Private Network (VPN)
* Personal Area Network (PAN)

**Types of Networks based on Topology:**

* Mesh Topology
* Ring Topology
* Bus Topology
* Star Topology
* Hybrid Topology
* Point to Point Topology

A picture containing diagram

Description automatically generated

**Cable Types:**

* **Coaxial Cabling**: Coaxial cable has an inner conductor that runs down the middle of the cable. This type of cabling comes in two types, thinnet and thicknet. Max Transmission Speed of 10 Mbps
* **Twisted-pair Cabling**: Has four pair of wires. It comes in two versions, UTP (Unshielded Twisted-Pair) and STP (Shielded Twisted-Pair). Uses 8P8C/RJ45 Connector
* **Fiber-optic Cabling**: Uses optical fibers to transmit data in the form of light signals. There are two types of fiber-optic cables - Single-mode fiber (SMF) and Multi-mode fiber (MMF). Uses ST/SC Connectors

Diagram

Description automatically generated with medium confidence

**Ethernet Standards:**

* **10Base-T** (IEEE 802.3): 10 Mbps with category 3 unshielded twisted pair (UTP) wiring, up to 100 meters long.
* **100Base-TX** (IEEE 802.3u): known as Fast Ethernet, uses category 5, 5E, or 6 UTP wiring, up to 100 meters long.
* **100Base-FX** (IEEE 802.3u): a version of Fast Ethernet that uses multi-mode optical fiber. Up to 412 meters long.
* **1000Base-CX** (IEEE 802.3z): uses copper twisted-pair cabling. Up to 25 meters long.
* **1000Base-T** (IEEE 802.3ab): Gigabit Ethernet that uses Category 5 UTP wiring. Up to 100 meters long.
* **1000Base-SX** (IEEE 802.3z): 1 Gigabit Ethernet running over multimode fiber-optic cable.
* **1000Base-LX** (IEEE 802.3z): 1 Gigabit Ethernet running over single-mode fiber.
* **10GBase-T** (802.3.an): 10 Gbps connections over category 5e, 6, and 7 UTP cables.

**Ethernet Cable Forms:**

* **Straight-through Cable:** On a straight through cable, the wired pins match. Straight through cable use one wiring standard: both ends use T568A wiring standard or both ends use T568B wiring standard.
* **Crossover Cable:** Crossover cable uses two different wiring standards: one end uses the T568A wiring standard, and the other end uses the T568B wiring standard. Pin1->Pin3 and Pin2->Pin6

Chart

Description automatically generated



**Data flow Types:**

* **Simplex Mode:** Communication is unidirectional.
* **Half-Duplex Mode:** Each station can both transmit and receive, but not at the same time.
* **Full-Duplex Mode:** Both stations can transmit and receive simultaneously.



**Communication Types:**

* **Unicast:** Communication from one point to another point
* **Broadcast:** Communication from one point to all other points
* **Multicast:** Communication from one/more points to a set of other points
* **Anycast:** It is a network addressing and routing methodology in which a single destination IP address is shared by nodes in multiple locations.

A picture containing clock, watch

Description automatically generated

**Domain:**

* **Broadcast Domain:** A broadcast domain is a logical division of a computer network, in which all nodes can reach each other by broadcast at the data link layer.
* **Collision Domain:** A collision domain is a network segment connected by a shared medium where simultaneous data transmissions collide with one another.



**54321 Rule:**

5 - the number of network segments

4 - the number of repeaters needed to join the segments into one collision domain

3 - the number of network segments that have active (transmitting) devices attached

2 - the number of segments that do not have active devices attached

1 - the number of collision domains

**Types of Layered Models: Layers and Protocol Data Units (PDUs):**

**OSI Model:**

* Physical Layer (Bits)
* Datalink Layer (Frame)
* Network Layer (Packet)
* Transport Layer (Segment)
* Session Layer (Data)
* Presentation Layer (Data)
* Application Layer (Data)

**TCP/IP Model (4):**

* Physical Layer (Frame): Physical Addresses (MAC)
* Network Layer (Packet): IP Addresses (IP)
* Transport Layer (Segment): Port Addresses (Ports)
* Application Layer (Data): Specific Addresses (Data)

**TCP/IP Model (5 – In use by CCNA):**

* Physical Layer (Bits)
* Datalink Layer (Frame): Physical Address (MAC)
* Network Layer (Packet): IP Addresses (IP)
* Transport Layer (Segment): Port Addresses (Ports)
* Application Layer (Data): Specific Addresses (Data)

**Cisco 3-Layer Model:**

* Access Layer: Controls User and Workgroup access to the resources on the network
* Distribution Layer: Serves as the communication point between the access layer and the core.
* Core Layer: Responsible for transporting large amounts of traffic quickly.

**Math Review:**

* Binary:
* IPv4 addresses use Binary.
* 2 possible values per bit (Base 2): 0,1
* Total number of outcomes for a given number: 2n (For example, for 8 bits: 28 = 256)
* To represent 255 in Binary

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Base | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 |
| Binary Bit | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| Decimal | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1 |

128+64+32+16+8+4+2+1 = 255

* IPv4 has 32 bits – 4 octets. 232 = 429,49,67,296 IP addresses
* Hexadecimal:
  + MAC addresses use Hexadecimal.
  + 16 possible values per bit (Base 16): 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, A, B, C, D, E, F
  + Converting from Decimal to Hexadecimal (Ex: 224->E0):

224 in Binary: 1110 0000 (Divide into 4 bits each)

11102 = 1410 = E16

00002 = 010 = 016

Result: E0

**IPv4 Addressing:**

* Internet Protocol v4 is a connectionless network layer protocol. Each packet is treated independently in this protocol which allows the packets to take different paths as needed.
* An IPv4 address is a layer 3 logical address assigned by an administrator. It is used to identify specific devices on a network and must be unique in internet.
* Private IP addresses are NATted to public address when traffic is sent onto internet.
* Format of IP address:
* 32 bits 4 octets of 8 bits (1byte) each
* Network Address Portion (Network ID)
  + - Identifies a specific network.
    - Routers look at destination of IP address and match to network address.
* Host portion (Host ID):
  + - Identifies a specific endpoint on a network.
* Address Classes to accommodate different sizes of network and aid in classifying networks:

|  |  |  |
| --- | --- | --- |
| Class A – Unicast | 0.0.0.0 to 127.255.255.255 | 8 network bits, 24 host bits |
| Class B – Unicast | 128.0.0.0 to 191.255.255.255 | 16 network bits, 16 host bits |
| Class C – Unicast | 192.0.0.0 to 223.255.255.255 | 24 network bits, 8 host bits |
| Class D – Multicast | 224.0.0.0 to 240.255.255.255 |  |
| Class E – Reserved for future | 241.0.0.0 to 255.255.255.255 |  |

* Exceptions, Reservations and Special addresses:
* 0.0.0.0/8 - Default network
* 127.0.0.0/8 – Local Loopback address.
* 224.0.0.X – Link local multicasts, generally used by routing tables.
* 224.0.0.5-224.0.0.6 - OSPF
* Directed Broadcast address: Fill 1s in the entire host portion of the address.
* Local Broadcast address: Fill 1s in all 32 bits. Generally used for DHCP address
* 10.0.0.0/8 – Private IP address range (not routable on internet)
* 172.16.0.0/12 – Private IP address range (not routable on internet)
* 192.168.0.0/16 – Private IP address range (not routable on internet)
* 169.254.0.0/16 – Non-routable Link Local Addresses (Automatic Private IP Addressing)
* Subnet Masks:
* Used to determine network and host portion of a given IP address through AND operation.
* Is the device remote (route through default gateway) or local (ARP)?
* Class A: 255.0.0.0
* Class B: 255.255.0.0
* Class C: 255.255.255.0
* Discontinuous subnet masks not supported:

*11110000.11111111.00000110.11000000 (240.244.3.191)*

* Only contiguous subnet masks are supported.

*11111111.11110000.00000000.00000000 (255.240.0.0)*

* Classless Inter Domain Routing (CIDR):
* Replaces classful IP addressing with variable length subnet mask (VLSM)
* CIDR notation /X where X denotes number of 1’s present in binary form of a subnet mask.
* Reduces wastage of big number of addresses.
* Ex: /11 = 255.224.0.0
* Subnetting:
  + Work the following for a given IP address: Network address, First IP address, Last IP address, Broadcast address.
  + Binary method to work an IP address:
    - Subnet address: Fill the host portion with binary 0s.
    - Broadcast address: Fill the host portion with binary 1s.
    - First host: Fill the host portion with binary 0s and set the last bit to 1.
    - Last host: Fill the host portion with binary 1s and set the last bit to 0.
    - Ex: 172.16.35.123/20:

Subnet: **172.16.0010** **0000.0000 0000** = 172.16.32.0

1st Host: **172.16.0010** **0000.0000 0001** = 172.16.32.1

Last Host: **172.16.0010** **1111.1111 1110** = 172.16.47.254

Broadcast: **172.16.0010** **1111.1111 1111** = 172.16.47.255

**Connecting to Networking Devices:**

* Connectors used: Serial Cable or RJ45 or USB.
* Protocols used: Telnet, SSH, GUI
* Review Cisco common CLI command reference

**TCP AND UDP PORT NUMBERS**

**ECHO                7/TCP**

**ECHO                7/UDP**

**FTP-DATA           20/TCP                           #FTP, DATA**

**FTP                21/TCP                           #FTP, CONTROL**

**SSH                22/TCP                           #SSH REMOTE LOGIN**

**TELNET             23/TCP**

**SMTP               25/TCP    MAIL**

TIME               37/TCP    TIMSERVER

TIME               37/UDP    TIMSERVER

RLP                39/UDP    RESOURCE               #RESOURCE LOCATION

NAMESERVER         42/TCP    NAME                   #HOST NAME SERVER

NAMESERVER         42/UDP    NAME                   #HOST NAME SERVER

NICNAME            43/TCP    WHOIS

**DNS                53/TCP                           #DOMAIN NAME SERVER**

**DNS                53/UDP                           #DOMAIN NAME SERVER**

**BOOTPS             67/UDP    DHCPS                  #BOOTSTRAP PROTOCOL**

**BOOTPC             68/UDP    DHCPC                  #BOOTSTRAP PROTOCOL**

**TFTP               69/UDP                           #TRIVIAL FILE TRANSFER**

**HTTP               80/TCP    WWW WWW-HTTP           #WORLD WIDE WEB**

KERBEROS           88/TCP    KRB5 KERBEROS-SEC      #KERBEROS

KERBEROS           88/UDP    KRB5 KERBEROS-SEC      #KERBEROS

RTELNET           107/TCP                           #REMOTE TELNET SERVICE

POP2              109/TCP    POSTOFFICE             #POST OFFICE PROTOCOL

**POP3              110/TCP                           #POST OFFICE PROTOCOL**

SQLSERV           118/TCP                           #SQL SERVICES

**NTP               123/UDP                           #NETWORK TIME PROTOCOL**

NETBIOS-NS        137/TCP    NBNAME                 #NETBIOS NAME SERVICE

NETBIOS-NS        137/UDP    NBNAME                 #NETBIOS NAME SERVICE

**IMAP              143/TCP    IMAP4                  #INTERNET MESSAGE**

**ACCESS PROTOCOL**

SQL-NET           150/TCP

SQLSRV            156/TCP

**SNMP              161/UDP                           #SNMP**

SNMPTRAP          162/UDP    SNMP-TRAP              #SNMP TRAP

BGP               179/TCP

**IRC               194/TCP                           #INTERNET RELAY CHAT**

MFTP              349/TCP

MFTP              349/UDP

**LDAP              389/TCP**

**HTTPS             443/TCP    MCOM                   #HTTP OVER TLS/SSL**

**HTTPS             443/UDP    MCOM                   #HTTP OVER TLS/SSL**

**ISAKMP            500/UDP    IKE                    #INTERNET KEY EXCHANGE**

CMD               514/TCP    SHELL

SYSLOG            514/UDP

ROUTER            520/UDP    ROUTE ROUTED

TIMED             525/UDP    TIMESERVER

DHCPV6-CLIENT     546/TCP                           #DHCPV6 CLIENT

DHCPV6-CLIENT     546/UDP                           #DHCPV6 CLIENT

DHCPV6-SERVER     547/TCP                           #DHCPV6 SERVER

DHCPV6-SERVER     547/UDP                           #DHCPV6 SERVER

**LDAPS             636/TCP    SLDAP                  #LDAP OVER TLS/SSL**

MSEXCH-ROUTING    691/TCP                           #MS EXCHANGE ROUTING

MSEXCH-ROUTING    691/UDP                           #MS EXCHANGE ROUTING

FTPS-DATA         989/TCP                           #FTP DATA,OVER TLS/SSL

FTPS              990/TCP                           #FTP CTRL OVER TLS/SSL

TELNETS           992/TCP                           #TELNET OVER TLS/SSL

**WINS             1512/TCP                           #WINDOWS NAME SERVICE**

**WINS             1512/UDP                           #WINDOWS NAME SERVICE**

**L2TP             1701/UDP**

**H.323     1718/TCP     #H.323 RAS (MULTICAST)**

**H.323     1719/TCP     #H.323 RAS (UNICAST)**

**H.323     1720/TCP     #H.323 CALL SIGNALLING**

**PPTP             1723/TCP                           #POINT-TO-POINT**

**TUNNELING PROTOCOL**

**RADIUS           1812/UDP                           #RADIUS AUTHENTICATION**

**SSO     2258/UDP                           #SINGLE SIGN OUT**

**RDP     3389/TCP     #REMOTE DESKTOP PROTOCOL**

MSFW-CONTROL     3847/TCP                           #MICROSOFT FIREWALL

SDP-PORTMAPPER   3935/TCP                           #SDP PORT MAPPER PROTOCOL

SDP-PORTMAPPER   3935/UDP                           #SDP PORT MAPPER PROTOCOL

**IPSEC            4500/TCP                           #MICROSOFT IPSEC NAT-T**

**IPSEC            4500/UDP                           #MICROSOFT IPSEC NAT-T**

**SIP     5060/UDP     #NON-ENCRYPTED TRAFFIC**

**SIP     5061/UDP     #SIP OVER TLS**

MS-LICENSING     5720/TCP                           #MICROSOFT LICENSING

MS-LICENSING     5720/UDP                           #MICROSOFT LICENSING

MAN              9535/TCP                           #REMOTE MAN SERVER

**IP PORT NUMBERS**

**IP               0     IP           # INTERNET PROTOCOL**

**ICMP             1     ICMP         # INTERNET CONTROL MESSAGE PROTOCOL**

GGP              3     GGP          # GATEWAY-GATEWAY PROTOCOL

**TCP              6     TCP          # TRANSMISSION CONTROL PROTOCOL**

EGP              8     EGP          # EXTERIOR GATEWAY PROTOCOL

PUP              12    PUP          # PARC UNIVERSAL PACKET PROTOCOL

**UDP              17    UDP          # USER DATAGRAM PROTOCOL**

HMP              20    HMP          # HOST MONITORING PROTOCOL

XNS-IDP          22    XNS-IDP      # XEROX NS IDP

RDP              27    RDP          # "RELIABLE DATAGRAM" PROTOCOL

**IPV6             41    IPV6         # INTERNET PROTOCOL IPV6**

IPV6-ROUTE       43    IPV6-ROUTE   # ROUTING HEADER FOR IPV6

IPV6-FRAG        44    IPV6-FRAG    # FRAGMENT HEADER FOR IPV6

**ESP              50    ESP          # ENCAPSULATING SECURITY PAYLOAD**

**AH               51    AH           # AUTHENTICATION HEADER**

IPV6-ICMP        58    IPV6-ICMP    # ICMP FOR IPV6

IPV6-NONXT       59    IPV6-NONXT   # NO NEXT HEADER FOR IPV6

IPV6-OPTS        60    IPV6-OPTS    # DESTINATION OPTIONS FOR IPV6

**Cisco Common CLI Reference**

|  |  |
| --- | --- |
| enable | Switch to enable mode from user mode |
| configure terminal | Switch to configure terminal mode from enable mode |
| disable | To go back to user mode |
| erase startup-config | Delete existing startup-config |
| show version | To see the version of the firmware installed |
| hostname | To change the hostname of the device |
| copy run start | Saving configuration to NVRAM |
| wr | Same function as copy run start |
| show ip int br | See interfaces on the router |
|  |  |